R5#show run
Building configuration...

Current configuration : 3847 bytes
!
! Last configuration change at 12:40:12 UTC Sun Jun 14 2020
!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R5
!
boot-start-marker
boot-end-marker
!
aqm-register-fnf
!
!
no aaa new-model
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
no ip icmp rate-limit unreachable
!
!
!
!
!
!
!
!

!
!
!
!
no ip domain lookup
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
redundancy
!
!
ip tcp synwait-time 5
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback1
 ip address 5.5.5.5 255.255.255.255
 ip ospf 1 area 0
!
interface Loopback10
 ip address 130.5.1.1 255.255.255.255
!
interface Loopback20
 ip address 130.5.2.1 255.255.255.255
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/0.45
 encapsulation dot1Q 45
 ip address 30.4.5.5 255.255.255.0
!
interface Ethernet0/0.57
 encapsulation dot1Q 57
 ip address 30.5.7.5 255.255.255.0
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Serial1/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial1/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial1/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial1/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/3
 no ip address
 shutdown
 serial restart-delay 0
!
router ospf 1
 router-id 5.5.5.5
 network 30.0.0.0 0.255.255.255 area 0
!
router bgp 345
 bgp router-id 5.5.5.5
 bgp log-neighbor-changes
 bgp confederation identifier 300
 bgp confederation peers 378
 neighbor 4.4.4.4 remote-as 345
 neighbor 4.4.4.4 update-source Loopback1
 neighbor 7.7.7.7 remote-as 378
 neighbor 7.7.7.7 disable-connected-check
 neighbor 7.7.7.7 update-source Loopback1
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
alias exec c config terminal
!
line con 0
 exec-timeout 0 0
 privilege level 15
 logging synchronous
line aux 0
 exec-timeout 0 0
 privilege level 15
 logging synchronous
line vty 0 4
 login
 transport input none
!
!
end

R5#